variant=attiny861at18
description=ATtiny861 @ 18.432 MHz  (external oscillator; BOD disabled)
sketch.upload=arduinoisp::avrisp::arduinoispfuse::avrispfuse
upload.maximum_size=8192
upload.maximum_ram=512
bootloader.low_fuses=0xA0
bootloader.high_fuses=0xD7
bootloader.extended_fuses=0x00
build.mcu=attiny861
build.f_cpu=18432000L
build.core=tiny
build.variant=attiny861at18
group=Tiny
family=avrtiny
version=0.6
revision=1
core=tiny
