variant=attiny861at16
description=ATtiny861 @ 16 MHz  (internal oscillator + pll; BOD disabled)
sketch.upload=arduinoisp::avrisp::arduinoispfuse::avrispfuse
upload.maximum_size=8192
upload.maximum_ram=512
bootloader.low_fuses=0xF1
bootloader.high_fuses=0xDD
bootloader.extended_fuses=0x01
build.mcu=attiny861
build.f_cpu=16000000L
build.core=tiny
build.variant=attiny861at16
group=Tiny
family=avrtiny
version=0.6
revision=1
core=tiny
