variant=attiny167_20
description=Optiboot ATtiny167 @ 20 MHz  (external oscillator; BOD enabled)
sketch.upload=arduino::arduinoispboot::avrispboot
#bootloader.upload=arduinoisp::avrisp
upload.speed=57600
upload.maximum_size=15808
upload.maximum_ram=512
bootloader.low_fuses=0xA0
bootloader.high_fuses=0xDF
bootloader.extended_fuses=0xFE
bootloader.path=optiboot
bootloader.file=optiboot_attiny167.hex
build.mcu=attiny167
build.f_cpu=20000000L
build.core=tiny
build.variant=attiny167_20
group=Tiny
family=avrtiny
version=0.6
revision=1
core=tiny
