variant=attiny84
description=Optiboot ATtiny84 @ 8 MHz  (internal osc)
sketch.upload=arduino::arduinoispboot::avrispboot
#bootloader.upload=arduinoisp::avrisp
upload.speed=19200
upload.maximum_size=7616
upload.maximum_ram=512
bootloader.low_fuses=0xE2
bootloader.high_fuses=0xD7
bootloader.extended_fuses=0xFE
bootloader.path=optiboot
bootloader.file=optiboot_attiny84.hex
build.mcu=attiny84
build.f_cpu=8000000L
build.core=tiny
build.variant=attiny84
group=Tiny
family=avrtiny
version=0.6
revision=1
core=tiny
