variant=attiny841_12-8
description=ATtiny841 @ 12.8 MHz  (internal osc)
sketch.upload=arduinoisp::avrisp::arduinoispfuse::avrispfuse
upload.maximum_size=8192
upload.maximum_ram=512
bootloader.low_fuses=0xE2
bootloader.high_fuses=0xD7
bootloader.extended_fuses=0xFE
build.mcu=attiny841
build.f_cpu=12800000L
build.core=tiny
build.variant=attiny841_12-8
group=Tiny
family=avrtiny
version=0.6
revision=1
core=tiny
