variant=attiny45at1
description=ATtiny45 @ 1 MHz  (internal oscillator; BOD disabled)
sketch.upload=arduinoisp::avrisp::arduinoispfuse::avrispfuse
upload.maximum_size=4096
upload.maximum_ram=256
bootloader.low_fuses=0x62
bootloader.high_fuses=0xD7
bootloader.extended_fuses=0xFF
build.mcu=attiny45
build.f_cpu=1000000L
build.core=tiny
build.variant=attiny45at1
group=Tiny
family=avrtiny
version=0.6
revision=1
core=tiny
