variant=attiny25at8
description=ATtiny25 @ 8 MHz  (internal oscillator; BOD disabled)
sketch.upload=arduinoisp::avrisp::arduinoispfuse::avrispfuse
upload.maximum_size=2048
upload.maximum_ram=128
bootloader.low_fuses=0xE2
bootloader.high_fuses=0xD7
bootloader.extended_fuses=0xFF
build.mcu=attiny25
build.f_cpu=8000000L
build.core=tiny
build.variant=attiny25at8
group=Tiny
family=avrtiny
version=0.6
revision=1
core=tiny
