variant=attiny4313at12
description=ATtiny4313 @ 12 MHz  (crystal; BOD disabled)
sketch.upload=arduinoisp::avrisp::arduinoispfuse::avrispfuse
upload.maximum_size=4096
upload.maximum_ram=256
bootloader.low_fuses=0xFF
bootloader.high_fuses=0xDF
bootloader.extended_fuses=0xFF
build.mcu=attiny4313
build.f_cpu=12000000L
build.core=tiny
build.variant=attiny4313at12
group=Tiny
family=avrtiny
version=0.6
revision=1
core=tiny
