variant=attiny24at16
description=ATtiny24 @ 16 MHz  (external crystal; BOD disabled)
sketch.upload=arduinoisp::avrisp::arduinoispfuse::avrispfuse
upload.maximum_size=2048
upload.maximum_ram=128
bootloader.low_fuses=0xFF
bootloader.high_fuses=0xD7
bootloader.extended_fuses=0xFF
build.mcu=attiny24
build.f_cpu=16000000L
build.core=tiny
build.variant=attiny24at16
group=Tiny
family=avrtiny
version=0.6
revision=1
core=tiny
